**MDF Rose Engine Lathe 2.0**

**with Stepper Motor Drive**

**A picture containing indoor, table, desk, sitting

Description automatically generated**

**Instructions for Building**

**Jigs, Fixtures, & Add-Ons**

**Version 1.0**

**24 March 2021**

This document is intended to help one familiar with the MDF rose engine to easily build the identified jigs, fixtures, and add-ons. You can purchase these from us at [www.ColvinTools.com](http://www.ColvinTools.com), or build them yourself.

As you get started with building these jigs, fixtures, or add-ons to the MDF rose engine lathe, please consider making the machine exactly according to the outlined instructions. There are lots of ways you can modify this, and, quite frankly, the MDF rose engine encourages experimentation. But it is best to attempt those modifications after understanding how it works. Some ideas which sound grand may not appear so after understanding how the machine works (we speak from experience).

If you have any questions on the terminology in this document, check out the “Ornamental Turning Book of Knowledge” ([www.OTBoK.info](https://www.otbok.info/)).

Throughout this document, I’ve tried to show the MDF in its native color of tan/brown. There are differences in the images I captured from the CAD drawing made, but those are not representative of the machine’s differences.

The added pieces are typically shown in different colors to ensure they stand out from the MDF rose engine lathe.

Unless otherwise noted, the MDF is ¾” thick.

If you have any questions, please contact us at [ColvinTools@Gmail.com](mailto:ColvinTools@Gmail.com).

Good luck and we hope you enjoy this machine as much as we.

Rich Colvin & Jack Zimmel

Permission is not granted to manufacture these for sale.

Table of Contents

[Amplitude Adjuster 4](#_Toc67493076)

[Bill of Materials 6](#_Toc67493077)

[AA1 – MDF Spacer Block 7](#_Toc67493078)

[AA2 – MDF AA Alignment Block 8](#_Toc67493079)

[AA3 – Horizontal Bar 9](#_Toc67493080)

[AA4 – Vertical Bar 9](#_Toc67493081)

[105 – AA Lever Arm Axle 10](#_Toc67493082)

[R1 – AA Rubber 11](#_Toc67493083)

[Assembly 13](#_Toc67493084)

[Using the AA 13](#_Toc67493085)

# Amplitude Adjuster

The amplitude adjuster for the MDF Rose Engine Lathe 2.0 is shown installed to the right.

Also shown are some extra rubbers. Note that the RS1 has been flipped 180° to open up more space.

Details for building this follow the bill of materials.



Graphical user interface

Description automatically generatedThis diagram shows the AA removed from the MDF Rose Engine Lathe 2.0.

## Bill of Materials

Parts required for building this are below.

| Item # | Item | Qty | Source | Source  Part Number | Comments |
| --- | --- | --- | --- | --- | --- |
|  | **MDF Parts** |  |  |  |  |
| AA1 | MDF Spacer Block | 1 |  |  |  |
| AA2 | MDF AA Alignment Block | 1 |  |  |  |
|  | **Machined Parts** |  |  |  |  |
| AA3 | Aluminum bar, ¼” x 1” | 1 |  |  | A piece 7 ¾” to 8” long is needed.  Used for the horizontal bar. |
| AA4 | Aluminum bar, ¼” x ¾” | 2 |  |  | Two pieces, 12 ½” to 13” long (each) are needed.  Used for the vertical bars. |
| R1 | Rubber, Pointed | 2 |  |  | Shape  Description automatically generated |
| R2 | Rubber, 2” Radius | 2 |  |  | A picture containing shape  Description automatically generated |
| R3 | Rubber, Flat | 2 |  |  | Square  Description automatically generated with low confidence |
|  | **Other Parts** |  |  |  |  |
| 101 | Carriage Bolts, ¼”-20, 4” long | 2 | McMaster-Carr | 93548A560 |  |
| 102 | Washer, ¼” | 8 | McMaster-Carr | 90107A029 |  |
| 103 | Lock Washer, ¼” | 1 | McMaster-Carr | 92146A029 |  |
| 104 | Nut, ¼”-20 | 5 | McMaster-Carr | 95505A601 |  |
| 105 | Bolt, ¼”-20 | 1 | McMaster-Carr | 90272A196 | Used as the axle for the vertical bars (AA4). Cut down per drawing on pg. 10). Need 1 ½” of unthreaded area. |
| 106 | Spacer, ¼” ID, ½” Long | 1 | McMaster-Carr | 92510A765 |  |
| 107 | Collar, ¼” ID | 1 | McMaster-Carr | 6432K12 |  |
| 108 | T-Track Bolt, ¼”-20, 2 ½” to 3” Long | 2 | McMaster-Carr |  |  |
| 109 | T-Track Nut, ¼”-20 | 2 | McMaster-Carr |  |  |
| 110 | Bolt, #8-32, 5/8” Long | 2 | McMaster-Carr | 90272A196 |  |
| 111 | Knurled Nut, #8-32 | 2 | McMaster-Carr | 92741A120 |  |

## AA1 – MDF Spacer Block

This spacer block is used to attach the AA to the headstock at the correct distance. You will need to drill two holes in H4L on the headstock to match the thru holes.



5 ¼”

2 7/8 ”

**Top View**



1 ½”

1 ½”

Holes drilled for ¼” bolts.

“G” bit recommended.

**Side View**

## AA2 – MDF AA Alignment Block

This is used to help keep the vertical bars aligned to the rosettes.



2 ”

3/8 ”

3/8 ”

3/8 ”

1/2 ”

3/4 ”

3/4 ”

5 3/4 ”

2 1/4 ”

1 3/8 ”

**Top View**



Holes drilled for ¼” bolts.

“G” bit recommended.

Center in slot for T-Track.

**Side View**

## AA3 – Horizontal Bar

The horizontal bar is made from 1” x ¼” aluminum bar.



Hole drilled for ¼” bolt.

“G” bit recommended.

½”

½”

4”

7 ¾”

## AA4 – Vertical Bar

The vertical bars are made from ¾” x ¼” aluminum bar. There are two of these.



½”

8”

Hole drilled for ¼” bolt.

“G” bit recommended.

Hole drilled for #8-32 bolt.

#18 bit recommended.

12 ½” to 13”

## 105 – AA Lever Arm Axle

This is made from a partially threaded bolt. It can be cut with a hack saw, but be sure to smooth off the end, and chamfer it.

The one specified has sufficient unthreaded space.



~1 ½”

End is smoothed and chamfered after cutting.

## Square Description automatically generated with medium confidenceR1 – AA Rubber

Two are needed at any one time. More can be made. The basic shape to start with is like shown to the right, with measurements below.



½”

¼”

¾”



2 3/8”

2 3/8”

Through hole drilled for #8-32 bolt. #18 bit recommended.

1 3/16”

3/8”

Partial hole drilled for head of #8-32 bolt. Needs to be > 0.350”. 3/8” Forstner bit recommended. Drill this first. The point marks where to drill the through hole. Depth of the partial hole is 0.100” to 1/8”.

**Flat Rubber**

**A picture containing text, businesscard

Description automatically generated**

**Pointed Rubber**

### Various Rubber Shapes

Some examples of rubber shapes are below. Others can be made to accomplish the desired results.

A picture containing text, indoor

Description automatically generated

|  |  |  |
| --- | --- | --- |
| **Pointed** | **Flat** | **Rounded**  **(2” Radius)** |

## Assembly

1. Drill the two holes needed in the headstock.
2. Attach the MDF Spacer Block (AA1) to the headstock using two carriage bolts with nuts and flat washers (#101, #102, & #104). The spacer block should be flush with the top of H4L.

**Looking from the back**

(H2 removed)



Nut

Flat Washer

MDF Spacer Block

Carriage Bolt

H4L

1. Attach the Axle (#105, cut as shown on pg. 10) to the Horizontal Bar (AA3) using two nuts (#104) and a lock washer (#103).
2. Add a flat washer (#102), one vertical arm (AA4), the spacer (#106), the 2nd vertical arm (AA4), and the collar (#107).



Lock Washer

Washer

Horizontal Bar

Vertical Bars

Nuts

Spacer

Collar

**Looking from the front**

## A picture containing text Description automatically generatedUsing the AA

1. Attach a rubber to each Vertical bar using an #8-32 bolt (#110) and a knurled nut (#111).
2. Attach the Horizontal bar to the MDF Spacer Block using two nuts and flat washers (#102 & #104). Ensure the vertical bars so that they are aligned with the front column (B3) on the MDF Rose Engine Lathe 2.0.
3. Add the MDF AA Alignment block (AA2) and hold it in place using two T-Track bolts (#108) and nuts (#109).



MDF AA Alignment Block

Front B3 Column

Vertical Bars

AA Rubbers

**Looking from the top**

MDF Alignment Block installed at the top of the front B3 column.

* If reducing amplification, install it at the top of B3.
* If increasing amplification, install it below the RS1 rubber support, but as high as possible so as not to interfere with the AA rubbers.